;;  ASA Linetype
;;  for Mechanical
;;  modify and added by ASA
;;  Faculty of Architecture, Silpakorn University.
;;  December 2005
;;


;;
;; COmplex Linetype


*CWS,Chilled Water Pipe ----CWS----CWS----
A,20,-2,["CWS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-6

*HWS,Hot Water Pipe ----HWS----HWS----
A,20,-2,["HWS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-6

*CDRNAF,Condensate Pipe ----CDRNAF----CDRNAF----
A,20,-2,["CDRNAF",NORMAL,S=2,R=0.0,X=-1,Y=-1],-12

*CONDWS,Condenser Water Pipe ----CONDWS----CONDWS----
A,20,-2,["CONDWS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-12

*DTS,Dual Temp Pipe ----DTS----DTS----
A,20,-2,["DTS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-6

*STEAM,Steam Pipe ----STEAM----STEAM----
A,20,-2,["STEAM",NORMAL,S=2,R=0.0,X=-1,Y=-1],-10

*REFRS,Sprinkler Pipe ----REFRS----REFRS----
A,20,-2,["REFRS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-10

*BRINES,Refrigeration Pipe ----BRINES----BRINES----
A,20,-2,["BRINES",NORMAL,S=2,R=0.0,X=-1,Y=-1],-11

*ACIDWS,Acid Waste Pipe ----ACIDWS----ACIDWS----
A,20,-2,["ACIDWS",NORMAL,S=2,R=0.0,X=-1,Y=-1],-11

